1. Before updating the firmware, please use an USB drive, and  copy the firmware zip file(EW.tar.xz) to the USB drive.
2. Insert the USB drive into the USB port of the leak detector.
3. Please follow the further steps described in the instruction manual.